TODO

 * Add Error checking to ALL THE THINGS -- none of the nextpi- CLI tools have it

 * Enable User Friendly Pi Booting

 * disable network updates of packages

 * disable linux trying to set volume on Next's DAC

 * Document NextDAC Device Tree Overlay source, and release
